4.6. The “Manage Interfaces” Dialog Box
Prev | Chapter 4. Capturing Live Network Data | Next

## 4.6. The “Manage Interfaces” Dialog Box

Figure 4.6. The “Manage Interfaces” dialog box

The “Manage Interfaces” dialog box initially shows the “Local Interfaces” tab, which lets you manage the following:

Show
  Whether or not to show or hide this interface in the welcome screen and the “Capture Options” dialog.
Friendly Name
  A name for the interface that is human readable.
Interface Name
  The device name of the interface.
Comment
  Can be used to add a descriptive comment for the interface.

The “Pipes” tab lets you capture from a named pipe. To successfully add a pipe, its associated named pipe must have already been created. Click + and type the name of the pipe including its path. Alternatively, Browse can be used to locate the pipe.

To remove a pipe from the list of interfaces, select it and press -.

On Microsoft Windows, the “Remote Interfaces” tab lets you capture from an interface on a different machine. The Remote Packet Capture Protocol service must first be running on the target platform before Wireshark can connect to it.

On Linux or Unix you can capture (and do so more securely) through an SSH tunnel.

To add a new remote capture interface, click + and specify the following:

Host
  The IP address or host name of the target platform where the Remote Packet Capture Protocol service is listening. The drop-down list contains the hosts that have previously been successfully contacted. The list can be emptied by choosing “Clear list” from the drop-down list.
Port
  Set the port number where the Remote Packet Capture Protocol service is listening on. Leave blank to use the default port (2002).
Null authentication
  Select this if you don’t need authentication to take place for a remote capture to be started. This depends on the target platform. This is exactly as secure as it appears, i.e., it is not secure at all.
Password authentication
  Lets you specify the username and password required to connect to the Remote Packet Capture Protocol service.

Each interface can optionally be hidden. In contrast to the local interfaces, they are not saved in the `preferences` file.

| Note
Make sure you have outside access to port 2002 on the target platform. This is the default port used by the Remote Packet Capture Protocol service.

To remove a host including all its interfaces from the list, select it and click the - button.

Prev | Up | Next
4.5. The “Capture Options” Dialog Box | Home | 4.7. The “Compiled Filter Output” Dialog Box