9.8. LTE
Prev | Chapter 9. Telephony | Next

## 9.8. LTE

### 9.8.1. LTE MAC Traffic Statistics Window

Statistics of the captured LTE MAC traffic. This window will summarize the LTE MAC traffic found in the capture.

Figure 9.5. The “LTE MAC Traffic Statistics” window

The top pane shows statistics for common channels. Each row in the middle pane shows statistical highlights for exactly one UE/C-RNTI. In the lower pane, you can see the for the currently selected UE/C-RNTI the traffic broken down by individual channel.

### 9.8.2. LTE RLC Graph Window

The LTE RLC Graph menu launches a graph which shows LTE Radio Link Control protocol sequence numbers changing over time along with acknowledgements which are received in the opposite direction.

| Note
That graph shows data of a single bearer and direction. The user can also launch it from the `RLC Statistics` window.

Figure 9.6. The RLC Graph window

The image of the RLC Graph is borrowed from the Wireshark wiki.

### 9.8.3. LTE RLC Traffic Statistics Window

Statistics of the captured LTE RLC traffic. This window will summarize the LTE RLC traffic found in the capture.

Figure 9.7. The “LTE RLC Traffic Statistics” window

At the top, the check-box allows this window to include RLC PDUs found within MAC PDUs or not. This will affect both the PDUs counted as well as the display filters generated (see below).

The upper list shows summaries of each active UE. Each row in the lower list shows statistical highlights for individual channels within the selected UE.

The lower part of the windows allows display filters to be generated and set for the selected channel. Note that in the case of Acknowledged Mode channels, if a single direction is chosen, the generated filter will show data in that direction and control PDUs in the opposite direction.

Prev | Up | Next
9.7. ISUP Messages Window | Home | 9.9. MTP3 Windows