D.2. tshark: Terminal-based Wireshark
Prev | Appendix D. Related command line tools | Next

## D.2. tshark: Terminal-based Wireshark

TShark is a terminal oriented version of Wireshark designed for capturing and displaying packets when an interactive user interface isn’t necessary or available. It supports the same options as `wireshark`. For more information on `tshark` consult your local manual page (`man tshark`) or the online version.

Help information available from `tshark`.

    TShark (Wireshark) 4.4.7 (v4.6.7rc0-0-g2167e12fc6f7)
    Dump and analyze network traffic.
    See https://www.wireshark.org for more information.

    Usage: tshark [options] ...

    Capture interface:
      -i <interface>, --interface <interface>
                               name or idx of interface (def: first non-loopback)
      -f <capture filter>      packet filter in libpcap filter syntax
      -s <snaplen>, --snapshot-length <snaplen>
                               packet snapshot length (def: appropriate maximum)
      -p, --no-promiscuous-mode
                               don't capture in promiscuous mode
      -I, --monitor-mode       capture in monitor mode, if available
      -B <buffer size>, --buffer-size <buffer size>
                               size of kernel buffer in MiB (def: 2MiB)
      -y <link type>, --linktype <link type>
                               link layer type (def: first appropriate)
      --time-stamp-type <type> timestamp method for interface
      -D, --list-interfaces    print list of interfaces and exit
      -L, --list-data-link-types
                               print list of link-layer types of iface and exit
      --list-time-stamp-types  print list of timestamp types for iface and exit

    Capture display:
      --update-interval        interval between updates with new packets, in milliseconds (def: 100ms)
    Capture stop conditions:
      -c <packet count>        stop after n packets (def: infinite)
      -a <autostop cond.> ..., --autostop <autostop cond.> ...
                               duration:NUM - stop after NUM seconds
                               filesize:NUM - stop this file after NUM KB
                                  files:NUM - stop after NUM files
                                packets:NUM - stop after NUM packets
    Capture output:
      -b <ringbuffer opt.> ..., --ring-buffer <ringbuffer opt.>
                               duration:NUM - switch to next file after NUM secs
                               filesize:NUM - switch to next file after NUM KB
                                  files:NUM - ringbuffer: replace after NUM files
                                packets:NUM - switch to next file after NUM packets
                               interval:NUM - switch to next file when the time is
                                              an exact multiple of NUM secs
                             printname:FILE - print filename to FILE when written
                                              (can use 'stdout' or 'stderr')
    Input file:
      -r <infile>, --read-file <infile>
                               set the filename to read from (or '-' for stdin)

    Processing:
      -2                       perform a two-pass analysis
      -M <packet count>        perform session auto reset
      -R <read filter>, --read-filter <read filter>
                               packet Read filter in Wireshark display filter syntax
                               (requires -2)
      -Y <display filter>, --display-filter <display filter>
                               packet displaY filter in Wireshark display filter
                               syntax
      -n                       disable all name resolutions (def: "mNd" enabled, or
                               as set in preferences)
      -N <name resolve flags>  enable specific name resolution(s): "mtndsNvg"
      -d <layer_type>==<selector>,<decode_as_protocol> ...
                               "Decode As", see the man page for details
                               Example: tcp.port==8888,http
      -H <hosts file>          read a list of entries from a hosts file, which will
                               then be written to a capture file. (Implies -W n)
      --enable-protocol <proto_name>
                               enable dissection of proto_name
      --disable-protocol <proto_name>
                               disable dissection of proto_name
      --only-protocols <protocols>
                               Only enable dissection of these protocols, comma
                               separated. Disable everything else
      --disable-all-protocols
                               Disable dissection of all protocols
      --enable-heuristic <short_name>
                               enable dissection of heuristic protocol
      --disable-heuristic <short_name>
                               disable dissection of heuristic protocol
    Output:
      -w <outfile|->           write packets to a pcapng-format file named "outfile"
                               (or '-' for stdout). If the output filename has the
                               .gz extension, it will be compressed to a gzip archive
      --capture-comment <comment>
                               add a capture file comment, if supported
      -C <config profile>      start with specified configuration profile
      --global-profile         use the global profile instead of personal profile
      -F <output file type>    set the output file type; default is pcapng.
                               an empty "-F" option will list the file types
      -V                       add output of packet tree        (Packet Details)
      -O <protocols>           Only show packet details of these protocols, comma
                               separated
      -P, --print              print packet summary even when writing to a file
      -S <separator>           the line separator to print between packets
      -x                       add output of hex and ASCII dump (Packet Bytes)
      --hexdump <hexoption>    add hexdump, set options for data source and ASCII dump
         all                   dump all data sources (-x default)
         frames                dump only frame data source
         ascii                 include ASCII dump text (-x default)
         delimit               delimit ASCII dump text with '|' characters
         noascii               exclude ASCII dump text
         help                  display help for --hexdump and exit
      -T pdml|ps|psml|json|jsonraw|ek|tabs|text|fields|?
                               format of text output (def: text)
      -j <protocolfilter>      protocols layers filter if -T ek|pdml|json selected
                               (e.g. "ip ip.flags text", filter does not expand child
                               nodes, unless child is specified also in the filter)
      -J <protocolfilter>      top level protocol filter if -T ek|pdml|json selected
                               (e.g. "http tcp", filter which expands all child nodes)
      -e <field>               field to print if -Tfields selected (e.g. tcp.port,
                               _ws.col.info)
                               this option can be repeated to print multiple fields
      -E<fieldsoption>=<value> set options for output when -Tfields selected:
         bom=y|n               print a UTF-8 BOM
         header=y|n            switch headers on and off
         separator=/t|/s|<char> select tab, space, printable character as separator
         occurrence=f|l|a      print first, last or all occurrences of each field
         aggregator=,|/s|<char> select comma, space, printable character as
                               aggregator
         quote=d|s|n           select double, single, no quotes for values
      -t (a|ad|adoy|d|dd|e|r|u|ud|udoy)[.[N]]|.[N]
                               output format of time stamps (def: r: rel. to first)
      -u s|hms                 output format of seconds (def: s: seconds)
      -l                       flush standard output after each packet
                               (implies --update-interval 0)
      -q                       be more quiet on stdout (e.g. when using statistics)
      -Q                       only log true errors to stderr (quieter than -q)
      -g                       enable group read access on the output file(s)
      -W n                     Save extra information in the file, if supported.
                               n = write network address resolution information
      -X <key>:<value>         eXtension options, see the man page for details
      -U tap_name              PDUs export mode, see the man page for details
      -z <statistics>          various statistics, see the man page for details
      --export-objects <protocol>,<destdir>
                               save exported objects for a protocol to a directory
                               named "destdir"
      --export-tls-session-keys <keyfile>
                               export TLS Session Keys to a file named "keyfile"
      --color                  color output text similarly to the Wireshark GUI,
                               requires a terminal with 24-bit color support
                               Also supplies color attributes to pdml and psml formats
                               (Note that attributes are nonstandard)
      --no-duplicate-keys      If -T json is specified, merge duplicate keys in an object
                               into a single key with as value a json array containing all
                               values
      --elastic-mapping-filter <protocols> If -G elastic-mapping is specified, put only the
                               specified protocols within the mapping file
      --temp-dir <directory>   write temporary files to this directory
                               (default: /tmp)
      --compress <type>        compress the output file using the type compression format

    Diagnostic output:
      --log-level <level>      sets the active log level ("critical", "warning", etc.)
      --log-fatal <level>      sets level to abort the program ("critical" or "warning")
      --log-domains <[!]list>  comma-separated list of the active log domains
      --log-fatal-domains <list>
                               list of domains that cause the program to abort
      --log-debug <[!]list>    list of domains with "debug" level
      --log-noisy <[!]list>    list of domains with "noisy" level
      --log-file <path>        file to output messages to (in addition to stderr)

    Miscellaneous:
      -h, --help               display this help and exit
      -v, --version            display version info and exit
      -o <name>:<value> ...    override preference setting
      -K <keytab>              keytab file to use for kerberos decryption
      -G [report]              dump one of several available reports and exit
                               default report="fields"
                               use "-G help" for more help

    Dumpcap can benefit from an enabled BPF JIT compiler if available.
    You might want to enable it by executing:
     "echo 1 > /proc/sys/net/core/bpf_jit_enable"
    Note that this can make your system less secure!

Prev | Up | Next
Appendix D. Related command line tools | Home | D.3. tcpdump: Capturing with “tcpdump” for viewing with Wireshark