11.14. SCCP users Table
Prev | Chapter 11. Customizing Wireshark | Next

## 11.14. SCCP users Table

Wireshark uses this table to map specific protocols to a certain DPC/SSN combination for SCCP.

This table is a user table, as described in Section 11.7, “User Accessible Tables”, with the following fields:

Network Indicator
  An Integer representing the network indicator for which this association is valid.
Called DPCs
  A range of integers representing the dpcs for which this association is valid.
Called SSNs
  A range of integers representing the ssns for which this association is valid.
User protocol
  The protocol that is carried over this association

Prev | Up | Next
11.13. PRES Users Context List | Home | 11.15. SMI (MIB and PIB) Modules