5.10. The Packet Format Frame
Prev | Chapter 5. File Input, Output, And Printing | Next

## 5.10. The Packet Format Frame

The packet format frame is also a part of the “Export Packet Dissections” and “Print” dialog boxes. You can use it to specify which parts of dissection are exported or printed.

Figure 5.18. The “Packet Format” frame

Each of the settings below correspond to the packet list, packet detail, and packet bytes in the main window.

Packet summary line
  Export or print each summary line as shown in the “Packet List” pane.
Packet details

  Export or print the contents of the “Packet Details” tree.

  All collapsed
    Export or print as if the “Packet Details” tree is in the “all collapsed” state.
  As displayed
    Export or print as if the “Packet Details” tree is in the “as displayed” state.
  All expanded
    Export or print as if the “Packet Details” tree is in the “all expanded” state.
Packet Bytes
  Export or print the contents of the “Packet Bytes” pane.
Each packet on a new page
  For printing and some export formats, put each packet on a separate page. For example, when exporting to a text file this will put a form feed character between each packet.
Capture information header
  Add a header to each page with capture filename and the number of total packets and shown packets.

Prev | Up | Next
5.9. The “Packet Range” Frame | Home | Chapter 6. Working With Captured Packets